**NOVATWIST® PLASTIC SCREW CAP CLOSURES**

**To Apply:**

1. Place one closure over the top of a screw top bottle.
2. Push down on the top of the closure until you hear 2 distinct “clicks”.
3. Turn the closure clockwise 2 &1/2 to 3 turns or until firmly tightened and locked in place.

If closure does not “lock” in place (stop turning) after 3 turns it is not pushed down far enough.

Stand bottle upright and push down on closure again until one click is heard. Then turn closure 2 turns clockwise and it should lock in place.

**To open: \*Important,** Do not turn just the top cap. Follow the below instructions:

**To open,** grasp the entire closure and turn counter clock wise until the top cap seal breaks away from the lower portion of the capsule.

Then, turn the top cap counter clockwise to open and pour the contents.

Enjoy!

----------------------------------------------------------------------------------------